Product name: 4U-IPC-610L-480T-14 slot rack-mount industrial control chassis

Chassis size: width 483 × depth 483 × height 175 (MM) (including mounting ears and handles)

Product color: industrial gray

Material: Environmentally friendly\fingerprint-resistant\high-quality SGCC galvanized sheet

Thickness: 1.2MM

Supported optical drive: 1 5.25'' optical drive bay

Product weight: Net weight 11.15KG\Gross weight 14.7KG

Support power supply: standard ATX power supply PS/2 power supply

Supported graphics cards: 14 full-height PCI straight slots AT rear window

Support hard disk: Support 3.5'' 3 + 2.5'' 2 hard disk slots

Supported fans: 2 12025 silent fans + dustproof mesh cover on the front panel

Panel: USB2.0*2\Power switch*1\Restart switch*1 Power indicator*1\HDD indicator*1 PS\2*1

Support motherboard: PCA motherboard 315x266MM backward compatible

Carton size: height 623×width 568×depth 295 (MM)

Graphics card length limit: 338MM \ Graphics card height limit 124MM (can reach 138MM after removing the crossbeam)

CPU height limit: 127MM (can reach 140MM when crossbeam is removed)

Packaging: Double-layer lid packaging

