Product name: MM-3U-3813WE industrial control server chassis

Product color: The box body is the original color of the material, and the front panel is black

Gross weight: 8KG(GW)

Material: high quality flat galvanized steel

Chassis size: D*W*H(mm)

380*482*133.2mm (including mounting ears)

Packing size: corrugated paper 56cm*51cm*18cm

Box thickness: 1.2MM

Expansion slot: Rear window removable

Supports 4 full-height card slots

Use the I/O shield that comes with the motherboard

Support power supply: ATX specification server power supply PS\2 power supply ordinary PC power supply

Support motherboard: CEB (12*10.5) ATX (12*9.6), MicroATX (9.6"*9.6"),

Mini-ITX (6.7"*6.7") 304*260mm backward compatible

Supported optical drive: 5.25'' CD-ROM drive slot *3

Does not support ultra-thin notebook CD-ROM

Supported hard disk: 7 3.5" HDD hard disk slots (can be replaced with 7 2.5" SSD hard disks)

Hard disk hot swap: not supported

Supported fans: 2 80mm*25mm fans

Panel: USB2.0*2\Power switch*1\Restart switch*1\Power indicator*1\HDD indicator*1

