Product Name: 19-inch IPC-610L-450 Hot-swappable 4U Rack Server Chassis

Chassis dimensions: 482mm (W) × 450mm (D) × 174mm (H) (including mounting ears and handles)

Product Color: Industrial Gray

Material: Environmentally friendly, fingerprint-resistant, high-quality SGCC galvanized sheet

Thickness: 1.2MM

Optical drive supported: None

Product weight: Net weight 10.35KG / Gross weight 12.15KG

Supported power supplies: Standard ATX power supply, PS/2 power supply

Supported graphics cards: 7 full-height PCI slots

Supported hard drives: Supports two 3.5'' hard drives or two 2.5'' hard drives for hot-swapping.

Supported fans: one 12cm fan and one 8cm fan on the front panel (silent fan + dust cover)

Panel: USB 2.0 *2, Power switch *1, Reset switch *1

Power indicator light *1, Hard drive indicator light *1, 1 PS/2

Supported motherboards: 12''*10.5'' (305*265MM) backward compatible motherboard slots (ATX\M-ATX\MINI-ITX motherboards)

Graphics card specifications: Maximum length 334mm, maximum height 127mm (144mm without crossbeams).

CPU height limit: 129mm (147mm after removing the crossbeam)

Carton dimensions: Height 585 × Width 561 × Depth 292 (mm)

