Product name: 2U-350T aluminum panel rack chassis

Chassis size: width 482 × depth 350 × height 88.5 (MM)

(Including hanging ears and handles)

Product color: Tech Black

Material: high quality SGCC flat galvanized steel

High-grade brushed aluminum panel

Thickness: Box 1.2MM

Support optical drive: No

Product weight: Net weight 4.72KG\Gross weight 5.93KG

Support power supply: standard ATX power supply PS/2 power supply

Support expansion: 4 half-height PCI slots\3 COM ports

Support hard disk: 1 2.5'' + 2 3.5'' hard disk slots

Supported fans: 2 front 8CM silent iron mesh fans

Panel: USB2.0*2\Large power switch*1\Large reset switch*1

Power indicator light*1\hard disk indicator light*1

Support motherboard: M-ATX\MINI-ITX motherboard

9.6''*9.6''(245*245MM downward compatible)

Carton size: height 205×width 472×depth 535 (MM)

Tips: CPU fan height limit is 67mm

Graphics card length limit 289mm \ Graphics card height limit 63mm
